xil_axi_read_beat

XIL AXI read beat object -Single bus beat for the READ channel. It inherits all the member and methods of xil_axi_resp_beat.

Functions
set_data_size

virtual function void set_data_size( |
input | xil_axi_uint | update
| );

Sets the data size of the xil_axi_read_beat

get_data_size
virtual function xil_axi_uint get_data_size();

Returns the data size of the xil_axi_read_beat

copy

function void copy( |
xil_axi_read_beat | rhs
| );

Copies the contents of the input xil_axi_read_beat to the current xil_axi_read_beat

my_clone
virtual function xil_axi_read_beat my_clone();

Clones the current xil_axi_read_beat and returns a handle to the new xil_axi_read_beat.

convert2string
virtual function string convert2string();

Returns string with last,data,size and user information of xil_axi_read_beat

new

function new( |
input | string | name | = | "xil_axi_read_beat"
| );

Constructor to create a new read beat